**Resetting your Air Source Heat Pump**

There may be some instances where a reset of your Air Source Heat Pump (ASHP) is required, such as, following a power outage.

Please follow the below steps to get the unit back up and running:

**Step 1**

* Turn off the indoor unit via the isolation switches
* Turn off the outdoor unit by turning the red dial beside the unit

**Wait for 5 minutes**

**Step 2** – Ensure this is completed in the below order

* Turn the indoor unit back on via the isolation switches
* Turn the outdoor unit back on